PPE & Safety Gear Inspections

**The First Mate is the HSE Officer aboard and is responsible for ordering personal protective equipment.**

|  |  |
| --- | --- |
| **Print First Mate’s Name Below** | **Date: 01-January-2021** |
|  |  |

***Inspection Summary***

**DIRECTIONS:** Have each department inspect the PPE it uses. Report any damaged PPE below and remove it from service. Destroy it if possible to prevent accidental use. List any items that need to be replaced so the First Mate can order them. Turn in completed inspections to the First Mate.

|  |  |  |  |
| --- | --- | --- | --- |
| **Department** | **PPE / Gear** | **Why removed from service- Description/ condition (broken, old, cracked, damaged)** | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
|  |  |  | |
| **Replacements ordered (type and amt):** | | |

**First Mate’s Signature \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

PPE/ Safety Gear Inspection Checklist

|  |  |  |
| --- | --- | --- |
| **Inspector name (Print):** | **Inspector Signature** | **Date (01 Jan 2021)** |
|  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Deck Department/**  **Nav/ Tech Department** | | How many in Good Condition? | **How many Need to replace** | N/A |
| **A** | Hard hats |  |  |  |
| **B** | Work vests |  |  |  |
| **C** | Impact resistant gloves |  |  |  |
| **D** | Safety glasses- clear |  |  |  |
| **E** | Safety glasses- tinted (daytime use) |  |  |  |
| **F** | Climbing harnesses for work at heights |  |  |  |
| **G** | Life jackets- over water operations |  |  |  |
| **H** | Rain gear |  |  |  |
| **I** | Face Shields- grinding |  |  |  |
| **J** | Ear muffs (with or without radio) for winch operations |  |  |  |
| **K** | Ear Plugs available |  |  |  |
| **L** | Nitrile gloves (for handling grease, lubricants, paint, OSPHO and other chemicals) |  |  |  |
| **Notes: Sufficient PPE available? PPE needed but not available?** | | | | |

PPE/ Safety Gear Inspection Checklist

|  |  |  |
| --- | --- | --- |
| **Inspector name (Print):** | **Inspector Signature** | **Date (01 Jan 2021)** |
|  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Engineering**  **Department** | | How many in Good Condition? | **How many Need to replace** | N/A |
| **A** | Hard hats |  |  |  |
| **B** | Work vests |  |  |  |
| **C** | Impact resistant gloves |  |  |  |
| **D** | Safety glasses- clear |  |  |  |
| **E** | Safety glasses- tinted (daytime use) |  |  |  |
| **F** | Rubber mats under electrical panels |  |  |  |
| **G** | Insulated gloves for electrical work |  |  |  |
| **H** | Face Shields- grinding |  |  |  |
| **I** | Ear muffs (with or without radio) for double hearing protection areas |  |  |  |
| **J** | Sufficient Lockout Tagout supplies |  |  |  |
| **K** | Ear plugs available |  |  |  |
| **L** | Nitrile gloves (for handling grease, lubricants, chemicals) |  |  |  |
| **M** | Flashlights- in place with strong batteries |  |  |  |
| **Notes: Sufficient PPE available? PPE needed but not available?** | | | | |